Data/hora: 06/06/2024 02:52:10

Provedor de dados: | 5
País: | France
Título: | Les essais mécaniques a la DCN, de l'eprouvette aux structures
Autores: | Hoarau, P.
Data: | 1992-12
Ano: | 1992
Palavras-chave: | Tests; Materials testing; Ship technology; Composite materials; Essai sur tronçon; Essai mécanique; Structure sandwich; Matériau composite.
Resumo: | In order to correctly dimension surface ship hulls made of organic matrix composites, the DCN carries out different kinds of mechanical testing: Quasi-static and dynamic. Sample size varies from small scale (for material selection) to large scale (for the choice of assembling technology between deck and hull). As often as possible, the DCN performs correlation studies between its experiments and existing numerical tools, in order to improve the accuracy of computer modelling.
Tipo: | Text
Idioma: | Francês
Identificador: | http://archimer.ifremer.fr/doc/1992/acte-1083.pdf
Editor: | Actes de colloques. Ifremer. Brest [ACTES COLLOQ. IFREMER.]. 1992
Relação: | http://archimer.ifremer.fr/doc/00000/1083/
Formato: | application/pdf