Data/hora: 06/06/2024 00:21:10

Provedor de dados: 	5	
País: 	France	
Título: 	Modélisation hydro-sédimentaire de la baie du Mont Saint-Michel	
Autores: 	Cayocca, Florence; Dussauze, Morgan; Le Hir, Pierre; Bassoullet, Philippe; Jestin, Herve.	
Data: 	2006-09-14	
Ano: 	2006	
Palavras-chave: 	Turbidité; Sédiments cohésifs; Modèle; Courant; Mont Saint Michel.	
Resumo: 	A numerical model for hydrodynamics and sediment transport is applied to Mont Saint Michel Bay, where ecological concerns are related to sediment transfers. Recent current datasets recorded on the tidal flat show the wind influence on the currents during neap tide. They are compared to model outputs. The simulation of sediment transfers driven by tides and waves accurately mimics the sediment repartition in the Bay.	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	http://archimer.ifremer.fr/doc/2006/acte-6274.pdf	
Editor: 	IX èmes Journées Nationales Génie Côtier-Génie Civil, Brest, 12-14 septembre 2006	
Relação: 	http://archimer.ifremer.fr/doc/00000/6274/	
Formato: 	application/pdf