Data/hora: 06/06/2024 10:38:52

Provedor de dados: 	5	
País: 	France	
Título: 	Study of the manoeuvrability and security of a trawl gear	
Autores: 	Marichal, Dominique; Vincent, Benoit.	
Data: 	2006-09-10	
Ano: 	2006	
Palavras-chave: 	Runge Kutta; Elasticity; Simulation; Model; Trawl doors; Hydrodynamic; Fishing gear; Runge Kutta; Elasticite; Simulation; Modèle; Panneaux de chalut; Hydrodynamique; Engin de pêche.	
Resumo: 	A complete method is presented for determining the static and dynamic behaviour of a fishing gear. The net, which is very flexible, is modelised by a set of rigid bars. The hydrodynamic forces, applied to each bar, are determined by combining and generalizing the Landweber and Morison hypothesis. A CFD method is used to calculate the forces on trawl doors. The fundamental principle of dynamics is completed with length equations expressing the elasticity of the bars. It leads to a set of second order non-linear differential equations, which is solved using a Runge-Kutta method. We will now present a few examples of the various applications of our works : the study of the trawl gear equilibrium in a uniform flow, an example of manoeuvrability (gyration of the trawl gear) and an application to security with the simulation of an obstruction.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/2006/acte-4612.pdf	
Editor: 	Wuxi, Chine, 10 - 14 septembre 2006 + Lorient, Octobre 2006	
Relação: 	http://archimer.ifremer.fr/doc/00000/4612/	
Formato: 	application/pdf