Data/hora: 09/06/2024 14:51:22

Provedor de dados: | Institutional Archive of Ifreme (ArchiMer)
País: | France
Título: | Description et fonctionnement d'une installation en circuit fermé destinée à l'élevage de larves et juvéniles de soles. Premiers résultats
Autores: | Alayse, J.p.; Lahaye, J.
Data: | 1979
Ano: | 1979
Palavras-chave: | Circuit fermé; Élevage; Sole; Closed system; Breeding; Sole.
Resumo: | The experimental unit used previously in our laboratory for the study of the effect of the photoperiod on the growth of flatfish was based on the use of tanks with separate recirculation systems. We modified it, connecting the different tanks to a single, more powerful recirculation system. This new unit comprised four different parts s - a biological filtar and an ultraviolet sterilizer. - a gravity operated water distribution system. - a series of 12 rearing tanks. - a piping system connecting the tank outlets to the biological filter. The total volume of the unit was 8 900 l. 200 l were changed every week. The main advantages of this new unit was that the quality of the water supplied to all tanks could be exactly the same, and that various parameters (salinity, pH, nitrites, nitrates) could be maintained at the same level all along the experiment. The unit was used in an investigation on the effect of different photo­periods on two batches of newly hatched soles (5 850 and 12 000 fish) and a batch of metamorphosed ones (840 fish).
Tipo: | Text
Idioma: | Francês

Identificador:

http://archimer.ifremer.fr/doc/00305/41664/40873.pdf

http://archimer.ifremer.fr/doc/00305/41664/

Editor: | Publications du Centre National pour l'Exploitation des Océans (CNEXO). Série : Actes de colloques, n° 7, 1979, pp. 239-254
Formato: | application/pdf

Fonte:

Centre National pour l’Exploitation des Océan, 1979

info:eu-repo/semantics/openAccess

restricted use