Data/hora: 01/06/2024 14:32:25

Provedor de dados: | Institutional Archive of Ifreme (ArchiMer)
País: | France
Título: | A comparison between sea-surface temperature-measurements from satellite noaa4 and from airborne radiometer aries
Autores: | Albuisson, M; Pontier, L; Wald, L.
Data: | 1979
Ano: | 1979
Palavras-chave: | Températures de surface; Télédétection; Sea surface temperatures; Remote sensing.
Resumo: | Measurements of sea surface temperatures (Sst) in the Gulf of Lions, obtained by the satellite "Noaa 4" sensor Vhrr and by the airborne radiometer "Aries", are presented and compared. The results reveal the reliability of the Vhrr data in the range 16-20. SOC, the degree of accuracy being within O. 5°C of the relative temperatures, despite a malfunctionning of the "Noaa 4" Vhrr.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/00323/43432/43082.pdf

http://archimer.ifremer.fr/doc/00323/43432/

Editor: | Gauthier-villars
Formato: | application/pdf
Fonte: | Oceanologica Acta (0399-1784) (Gauthier-villars), 1979 , Vol. 2 , N. 1 , P. 1-4

Fonte:

info:eu-repo/semantics/openAccess

restricted use