Data/hora: 11/06/2024 16:49:45

Provedor de dados: | Institutional Archive of Ifreme (ArchiMer)
País: | France
Título: | An oceanographic grid system for coastal and continental margin areas
Autores: | Le Gall, Jean-yves.
Data: | 1974
Ano: | 1974
Palavras-chave: | Histoire Ifremer.
Resumo: | In the Marsden Square Grid System, or its derivations - and this is the system that most national and international oceanographic data acquisition centres employ  - the information is located geographically for statistical purposes by means of a grid consisting of 10°, 5° or 1° " squares ".  The system, an early one dating from 1850, has three major disadvantages, and this has meant that its numbering principle cannot be used for a grid whose smallest lattice is less than 1° of latitude by 1° of longitude. [NOT CONTROLLED OCR]
Tipo: | Text
Idioma: | Inglês
Identificador: | http://archimer.ifremer.fr/doc/1974/publication-5157.pdf
Editor: | Bureau hydrographique international
Relação: | http://archimer.ifremer.fr/doc/00000/5157/
Formato: | application/pdf
Fonte: | International Hydrographic Revue (Bureau hydrographique international), 1974 , Vol. 51 , N. 1 , P. 191-196
Fonte: | Bureau hydrographique international