Data/hora: 06/06/2024 04:45:07

Provedor de dados: | Institutional Archive of Ifreme (ArchiMer)
País: | France
Título: | Endommagement mecanique de materiaux composites. Role sur les proprietes hygrothermiques
Autores: | Perreux, D; Suri, C; Varchon, D; Oytana, C.
Data: | 1992-12
Ano: | 1992
Palavras-chave: | Moisture; Damage; Modelling; Ship technology; Mechanical properties; Composite materials; Humidité; Endommagement; Modélisation; Comportement; Matériau composite.
Resumo: | The mechanical behaviour of polymer based glass fibre composites depends on the damage level and the amount of moisture present. Two anelastic damage models, both adapted to the mechanical properties of epoxy and polyester matrix polymers, are proposed. A coupling effect between the kinetics of damage and moisture level is shown.
Tipo: | Text
Idioma: | Francês
Identificador: | http://archimer.ifremer.fr/doc/1992/acte-1062.pdf
Editor: | Actes de colloques. Ifremer. Brest [ACTES COLLOQ. IFREMER.]. 1992
Relação: | http://archimer.ifremer.fr/doc/00000/1062/
Formato: | application/pdf