Data/hora: 09/06/2024 06:34:00

Provedor de dados: 	5	
País: 	France	
Título: 	Evaluation of a lifetime-based optode to measure oxygen in aquatic systems	
Autores: 	Tengberg, A; Hovdenes, J; Andersson, H; Brocandel, O; Diaz, R; Hebert, D; Arnerich, T; Huber, C; Kortzinger, A; Khripounoff, Alexis; Rey, F; Ronning, C; Schimanski, J; Sommer, S; Stangelmayer, A.	
Data: 	2006-02	
Ano: 	2006	
Palavras-chave: 	Lifetime based optode; Measure; Oxygen; Aquatic systems.	
Resumo: 	In this article, we evaluate the performance of a commercially available lifetime-based optode and compare it with data obtained by other methods. We performed a set of 10 different tests, including targeted laboratory evaluations and field studies, covering a wide range of situations from shallow coastal waters and wastewater treatment plants to abyssal depths. Our principal conclusion is that, owing to high accuracy (+/- 2 mu M), long-term stability (more than 20 months), lack of pressure hysteresis, and limited cross-sensitivity, this method is overall more suitable for oxygen monitoring than other methods.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/2006/publication-1413.pdf	
Editor: 	ASLO	
Relação: 	http://archimer.ifremer.fr/doc/00000/1413/	
Formato: 	application/pdf	
Fonte: 	Limnology and Oceanography methods (depuis 2003) (ASLO), 2006-02 , Vol. 4 , P. 7-17	
Fonte: 	2006 by the American Society of Limnology and Oceanography Inc.