Data/hora: 01/06/2024 00:51:40

Provedor de dados: 	Institutional Archive of Ifreme (ArchiMer)	
País: 	France	
Título: 	Materiaux composites courants: Tenue au feu	
Autores: 	Croquette, Jean; Baudin, M.	
Data: 	1992-12	
Ano: 	1992	
Palavras-chave: 	Pipes; Fire; Tests; Materials testing; Ship technology; Composite materials; Tuyauteries; Sandwich; Tenue au feu; Matériau composite.	
Resumo: 	In the national naval composites project, several series of fire tests have been carried out on epoxy glass pipes and different structural materials commonly used in naval construction. This paper describes the materials tested and the procedures chosen to evaluate the fire reaction properties: flammability (M classification), smoke emission (F classification), and the fire resistance (IMO A 517(13)). The conclusions are given for both the testing procedures and the performance of the composite materials.	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	http://archimer.ifremer.fr/doc/1992/acte-1047.pdf	
Editor: 	Actes de colloques. Ifremer. Brest [ACTES COLLOQ. IFREMER.]. 1992	
Relação: 	http://archimer.ifremer.fr/doc/00000/1047/	
Formato: 	application/pdf