Data/hora: 02/06/2024 05:13:40

Provedor de dados: 	5	
País: 	France	
Título: 	Un modèle asymptotique de la plaque stratifiée	
Autores: 	Kail, R; Lene, F; De Roeck, Y.	
Data: 	1992-12	
Ano: 	1992	
Palavras-chave: 	Ship technology; Modelling; Mathematical models; Composite materials; Eléments finis; Développement asymptotique; Composites; Plaque.	
Resumo: 	In order to calculate the behaviour of thin structures of laminated composite materials, a bidimensional plate model is generated by an asymptotic development technique. From a structural analysis by plane finite elements at the middle surface, this model yields the equations leading to the computation, at each point of the laminated material, of the displacement and the stress tensor. After describing the theoretical model, numerical results are compared with the analytical solution of a test problem.	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	http://archimer.ifremer.fr/doc/1992/acte-1081.pdf	
Editor: 	Actes de colloques. Ifremer. Brest [ACTES COLLOQ. IFREMER.]. 1992	
Relação: 	http://archimer.ifremer.fr/doc/00000/1081/	
Formato: 	application/pdf