Data/hora: 10/06/2024 16:12:11

Provedor de dados: 	52	
País: 	Brazil	
Título: 	A computational fluid dynamics study of hydrogen bubbles in an electrochemical reactor	
Autores: 	Cavalcanti,Renata da Silva; Farias Neto,Severino Rodrigues de; Vilar,Eudésio Oliveira.	
Data: 	2005-06-01	
Ano: 	2005	
Palavras-chave: 	Hydrogen; Bubble; CFD; Finite volumes; Electrochemical reactor.	
Resumo: 	Most electrochemical reactors present reactions with the growth and departure of gas bubbles which influence on the reactor hydrodynamics and this study is usually complex, representing a vast field for research. The present paper had as objective to study a bi-phase (gas-liquid) system aiming to foresee the influence of departure of hydrogen bubbles generated on effective electrode surface situated on cathodic semi-cell. Nevertheless, it was idealized that the gas was injected into the semi cell, through the effective electrode surface With this hypothesis, it was possible to study, and numerically analyze, the hydrodynamic behavior of the hydrogen bubbles in the interior of the study domain, applying concepts of computational fluid dynamics by using the computational applicative CFX-4 for the application of the MUSIG ("MUltiple-SIze-Group") model, taking into consideration the phenomena of coalescence and the distribution of the diameter of the bubbles.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-89132005000400027	
Editor: 	Instituto de Tecnologia do Paraná - Tecpar	
Relação: 	10.1590/S1516-89132005000400027	
Formato: 	text/html	
Fonte: 	Brazilian Archives of Biology and Technology  v.48 n.spe 2005	
Fonte: 	info:eu-repo/semantics/openAccess