Data/hora: 09/06/2024 10:42:10

Provedor de dados: 	Brazilian Journal of Microbiology	
País: 	Brazil	
Título: 	Biomethane production from vinasse in upflow anaerobic sludge blanket reactors inoculated with granular sludge	
Autores: 	Barros,Valciney Gomes de; Duda,Rose Maria; Oliveira,Roberto Alves de.	
Data: 	2016-09-01	
Ano: 	2016	
Palavras-chave: 	Biogas; Mesophilic anaerobic treatment; Methane; Organic loading rate; Startup.	
Resumo: 	ABSTRACT The main objective of this study was to evaluate the anaerobic conversion of vinasse into biomethane with gradual increase in organic loading rate (OLR) in two upflow anaerobic sludge blanket (UASB) reactors, R1 and R2, with volumes of 40.5 and 21.5 L in the mesophilic temperature range. The UASB reactors were operated for 230 days with a hydraulic detection time (HDT) of 2.8 d (R1) and 2.8-1.8 d (R2). The OLR values applied in the reactors were 0.2-7.5 g totalCOD (L d)−1 in R1 and 0.2-11.5 g totalCOD (L d)−1 in R2. The average total chemical oxygen demand (totalCOD) removal efficiencies ranged from 49% to 82% and the average conversion efficiencies of the removed totalCOD into methane were 48-58% in R1 and 39-65% in R2. The effluent recirculation was used for an OLR above 6 g totalCOD (L d)−1 in R1 and 8 gtotalCOD (L d)−1 in R2 and was able to maintain the pH of the influent in R1 and R2 in the range from 6.5 to 6.8. However, this caused a decrease for 53-39% in the conversion efficiency of the removed totalCOD into methane in R2 because of the increase in the recalcitrant COD in the influent. The largest methane yield values were 0.181 and 0.185 (L) CH4 (gtotal COD removed)−1 in R1 and R2, respectively. These values were attained after 140 days of operation with an OLR of 5.0-7.5 g totalCOD (L d)−1 and total COD removal efficiencies around 70 and 80%.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1517-83822016000300628	
Editor: 	Sociedade Brasileira de Microbiologia	
Relação: 	10.1016/j.bjm.2016.04.021	
Formato: 	text/html	
Fonte: 	Brazilian Journal of Microbiology  v.47 n.3 2016	
Fonte: 	info:eu-repo/semantics/openAccess