Data/hora: 12/06/2024 15:29:34

Provedor de dados: | 63
País: | Brazil
Título: | On simple methods for unsaturated soil hydraulic conductivity determination
Autores: | Bacchi,O.O.S.; Reichardt,K.
Data: | 1993-09-01
Ano: | 1993
Palavras-chave: | Soil hydraulic conductivity; Unit gradient.
Resumo: | The simple methods of LIBARDI et al. (1980) and SISSON et al. (1980) for K(theta) estimation, although developed on completely different theoretical basis, are rigorously identical for the exponential hydraulic conductivity model. The unit gradient approximation used in these methods seems valid for practical purposes but is theoretically in valid.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90161993000200022
Editor: | São Paulo - Escola Superior de Agricultura "Luiz de Queiroz"
Relação: | 10.1590/S0103-90161993000200022
Formato: | text/html
Fonte: | Scientia Agricola  v.50 n.2 1993
Fonte: | info:eu-repo/semantics/openAccess