Data/hora: 02/06/2024 12:16:57

Provedor de dados: | 64
País: | Brazil
Título: | Aeration frequency on accelerated composting of animal carcasses
Autores: | Oliveira,Matias Marchesan de; Coldebella,Arlei; Belli Filho,Paulo; Oliveira,Paulo Armando Victória de.
Data: | 2018-12-01
Ano: | 2018
Palavras-chave: | Rotary drum reactor; Poultry and pig; Gas emission.
Resumo: | ABSTRACT Rotary drum reactors (RDRs) for accelerated carcass composting are being installed in animal production units as an alternative for the disposal of pig and poultry carcasses in Brazil. The aim of the present study was to investigate the influence of aeration frequency on gas emissions (CO2-C, CH4-C, NH3-N and N2O-N) during composting of pig and poultry carcasses in RDRs. RDRs with a volume of 3.6 m3 (50% useful volume) were used. Aeration time was 24 minutes. Four intervals between aeration periods were tested (treatments) as follows: 1 hour (T1), 2 hours (T2), 3 hours (T3) and 4 hours (T4). Gas emissions were continuously monitored using a photoacoustic gas monitor (INNOVA 1412). Temperature was monitored using iButtons mixed with the biomass. Mathematical models of CO2-C and NH3-N emissions relative to the observed biomass temperature were proposed. Biomass temperature was affected by the treatments. The highest aeration frequency had the shortest thermophilic phase (&gt;50 °C). No significant differences in total gas emissions were observed between treatments (p&gt;0.05). CO2-C and NH3-N emissions were better fitted by non-linear models (R2=0.75 and R2=0.78, respectively). A minimum 2-hour interval should be adopted between aeration periods of 24 minutes to guarantee a longer thermophilic phase and elimination of possible pathogenic contaminants.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1413-70542018000600653
Editor: | Editora da Universidade Federal de Lavras
Relação: | 10.1590/1413-70542018426021818
Formato: | text/html
Fonte: | Ciência e Agrotecnologia  v.42 n.6 2018
Fonte: | info:eu-repo/semantics/openAccess