Data/hora: 13/06/2024 23:38:35

Provedor de dados: 	69	
País: 	Chile	
Título: 	Effect of temperature and initial pH on biohydrogen production from palm oil mill effluent: long-term evaluation and microbial community analysis	
Autores: 	O-Thong,Sompong; Mamimin,Chonticha; Prasertsan,Poonsuk.	
Data: 	2011-09-01	
Ano: 	2011	
Palavras-chave: 	Biohydrogen; Long-term evaluation; Palm oil mill effluent; Response surface methodology; Thermophilic condition.	
Resumo: 	Anaerobic sludge from palm oil mill effluent (POME) treatment plant was used as a source of inocula for the conversion of POME into hydrogen. Optimization of temperature and initial pH for biohydrogen production from POME was investigated by response surface methodology. Temperature of 60ºC and initial pHof 5.5 was optimized for anaerobic microflora which gave a maximum hydrogen production of 4820 ml H2/l-POME corresponding to hydrogen yield of 243 ml H2/g-sugar. Total sugar consumption and chemical oxygen demand (COD) removal efficiency were 98.7% and 46%, respectively. Long-term hydrogen production in continuous reactor at HRT of 2 days, 1 day and 12 hrs were 4850 ± 90, 4660 ± 99 and 2590 ± 120 ml H2/l-POME, respectively. Phylogenetic analysis of the mixed culture revealed that members involved hydrogen producers in both batch and continuous reactors were phylogenetically related to the Thermoanaerobacterium thermosaccharolyticum. Batch reactor showed more diversity of microorganisms than continuous reactor. Microbial community structure of batch reactor was comprised of T. thermosaccharolyticum, T. bryantii, Thermoanaerobacterium sp., Clostridium thermopalmarium and Clostridium NS5-4, while continuous reactor was comprised of T. thermosaccharolyticum, T. bryantii and Thermoanaerobacterium sp. POME is good substrate for biohydrogen production under thermophilic condition with Thermoanaerobacterium species play an important role in hydrogen fermentation.	
Tipo: 	Journal article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.cl/scielo.php?script=sci_arttext&pid=S0717-34582011000500009	
Editor: 	Pontificia Universidad Católica de Valparaíso	
Formato: 	text/html	
Fonte: 	Electronic Journal of Biotechnology  v.14 n.5 2011