Data/hora: 16/06/2024 19:37:54

Provedor de dados: | 70
País: | Brazil
Título: | Evaluation of the effect of the seed extract of Moringa oleifera Lam over the efficiency of organic filters in wastewater treatment of dairy cattle breeding
Autores: | Francisco,João P.; Silva,Jonathas B. G.; Roque,Odir C. C.; Nascentes,Alexandre L.; Silva,Leonardo D. B.
Data: | 2014-02-01
Ano: | 2014
Palavras-chave: | Coagulant; Fertigation; Water treatment.
Resumo: | This study aimed to evaluate the effect of Moringa oleifera Lam extract on the removal of total solids (TS), total suspended solids (TSS) and chemical oxygen demand (COD), in different filter media for treating wastewater of dairy cattle breeding (DCW). The moringa seed extract was obtained by grinding 50 g of seeds in one liter of distilled water and, after passing the solution through a quantitative paper filter of 25 microns, 60 mL of the extract were added to wastewater from cattle breeding before the filtration process in organic filters made of thin coal, bamboo leaves, eucalyptus leaves, gliricidia branches and sawdust. This was followed by the completely randomized experimental design, adopting a factorial of 5 x 2. Aliquots of filtered effluent were collected and the total solids (TS) concentrations, total suspended solids (TSS) and chemical oxygen demand (COD) were determined. It was found that the increase in the efficiency of removal of COD and total solids can be attributed to the coagulating power of the moringa seed extract, wherein the filter medium with bamboo leaves presented the best performance, showing potential for use as alternative filter material in the primary treatment of DCW.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100015
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/S0100-69162014000100015
Formato: | text/html
Fonte: | Engenharia Agrícola  v.34 n.1 2014
Fonte: | info:eu-repo/semantics/openAccess