Data/hora: 03/06/2024 05:23:24

Provedor de dados: | 70
País: | Brazil
Título: | GRANULOMETRY AND ENERGY CONSUMPTION AS INDICATORS OF DISINTEGRATION EFFICIENCY IN A HAMMER MILL ADAPTED TO EXTRACTING ARROWROOT STARCH (Maranta arundinacea) IN COMPARISON TO STARCH EXTRACTION FROM CASSAVA
Autores: | Branco,Fabiano P.; Naka,Marco H.; Cereda,Marney P.
Data: | 2019-06-01
Ano: | 2019
Palavras-chave: | Appropriate Technology; Small producers; Mechanization; Agribusiness.
Resumo: | ABSTRACT The commercial sector of starch extraction has fully automated plants with a minimum scale of 200 ton.day–1, which extracts starch from maize and cassava in Brazil. Although these starches are commodities, the market demands starches with special properties obtained without chemical modifications. A higher-priced starch can compensate for small-scale extraction, as in the case of arrowroot starch, which would correspond to an alternative income for the producer. As a small-scale equipment was not available in Brazil, it was necessary to adapt a hammer mill for arrowroot starch extraction, which should have a performance similar to that obtained from cassava roots using industrial grinders. The degree of disintegration and energy consumption were adopted as the efficiency indexes. The hammer mill was equipped with two perforated plates. The results showed that use of an adapted hammer mill provides an average diameter of 74.64 ± 0.09 μm for perforated plate 1 (TP1) and 76.62 ± 0.06 μm for TP2; these results were equivalent to those obtained with cassava in the respective perforations which, in turn, was comparable to the degree of grinding obtained with large industrial equipment. The specific energy consumption needs for arrowroot disintegration varied from 31.47 to 48.91 kJ.kg–1, which was considered close to that calculated for large-scale industrial cassava roots grinders, reported at 37.03 kJ.kg–1.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300341
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/1809-4430-eng.agric.v39n3p341-349/2019
Formato: | text/html
Fonte: | Engenharia Agrícola  v.39 n.3 2019
Fonte: | info:eu-repo/semantics/openAccess