Data/hora: 11/06/2024 06:51:38

Provedor de dados: 	70	
País: 	Brazil	
Título: 	INFLUENCE OF FATIGUE ON BENDING OF Pinus caribaea WOOD	
Autores: 	Christoforo,André L.; Barbosa,Thaina Q.; Almeida,Diego H. de; Panzera,Tulio H.; Lahr,Francisco A. R.	
Data: 	2020-04-01	
Ano: 	2020	
Palavras-chave: 	Fatigue; Pinus caribaea; Static bending; Analysis of variance; Regression models.	
Resumo: 	ABSTRACT This research aimed to evaluate the effect of the number of fatigue cycles (NC, 0 – reference, 450, 4500, 45000, and 90000) for frequencies (Fr) of oscillation equal to 0.5 and 1.0 Hz on the modulus of elasticity (Em) and operating stress (σm) in the static bending of Pinus caribaea wood. Em and σm were determined taking into account three specimens (SPEC) manufactured for reference condition and another three for each of the four NC levels and each Fr level, resulting in 27 SPEC. Sixty experimental determinations were obtained, being the approximate total time of sample exposure to fatigue of 350 hours. The same specimens used to determine Em and σm for the reference condition were also used (via non-destructive tests) to obtain these properties for all fatigue cycles. The frequency and number of cycles significantly influenced both investigated properties. Reductions in Em and σm values were observed after 45000 cycles. The progressive increase in the number of fatigue cycles caused more marked reductions in mechanical properties when compared to the increase in the frequency of oscillation.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200238	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/1809-4430-eng.agric.v40n2p238-242/2020	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.40 n.2 2020	
Fonte: 	info:eu-repo/semantics/openAccess