Data/hora: 16/06/2024 17:45:39

Provedor de dados: 	91	
País: 	Brazil	
Título: 	Characterization of venturi injector using dimensional analysis	
Autores: 	Sobenko,Luiz R.; Frizzone,José A.; Camargo,Antonio P. de; Saretta,Ezequiel; Rocha,Hermes S. da.	
Data: 	2019-07-01	
Ano: 	2019	
Palavras-chave: 	Buckinghan Pi theorem; Irrigation equipment; Fertigation.	
Resumo: 	ABSTRACT Venturi injectors are commonly employed for fertigation purposes in agriculture, in which they draw fertilizer from a tank into the irrigation pipeline. The knowledge of the amount of liquid injected by this device is used to ensure an adequate fertigation operation and management. The objectives of this research were (1) to carry out functional tests of Venturi injectors following requirements stated by ISO 15873; and (2) to model the injection rate using dimensional analysis by the Buckingham Pi theorem. Four models of Venturi injectors were submitted to functional tests using clean water as motive and injected fluid. A general model for predicting injection flow rate was proposed and validated. In this model, the injection flow rate depends on the fluid properties, operating hydraulic conditions and geometrical characteristics of the Venturi injector. Another model for estimating motive flow rate as a function of inlet pressure and differential pressure was adjusted and validated for each size of Venturi injector. Finally, an example of an application was presented. The Venturi injector size was selected to fulfill the requirements of the application and the operating conditions were estimated using the proposed models.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662019000700484	
Editor: 	Departamento de Engenharia Agrícola  - UFCG	
Relação: 	10.1590/1807-1929/agriambi.v23n7p484-491	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Engenharia Agrícola e Ambiental  v.23 n.7 2019	
Fonte: 	info:eu-repo/semantics/openAccess