Consulta: creatorFacets:"Lucas,Fidel C. B."
Registros recuperados: 2
Data/hora: 04/06/2024 05:23:46

Uso de mesa vertical como parâmetro para regulagens de turboatomizadores
Provedor de dados: 70
Autores: Mion,Renildo L.; Sombra,Weberte A.; Duarte,José M. de L.; Nascimento,Elivânia M. S.; Viliotti,Carlos A.; Lucas,Fidel C. B.; Monte,Clesson A.
O consumo excessivo de agrotóxicos na agricultura brasileira é preocupante, e um dos fatores que contribuem para este excesso é o uso incorreto dos equipamentos de aplicação, causando grandes problemas de contaminação ambiental. O sucesso de uma aplicação agrícola somente é efetivado quando se consegue atingir o alvo com a menor contaminação ambiental possível. O objetivo deste trabalho foi comparar o perfil da distribuição vertical de um turboatomizador com e sem fluxo de ar e o número de bicos utilizados nos ramais, utilizando-se de uma mesa vertical como parâmetro de avaliação. O conjunto utilizado foi um trator marca VALTRA, modelo BM-120 4x2 TODA, e um turboatomizador da marca Jacto, modelo ARBUS 400 GOLDEN, com pontas do tipo J5-2, pressão de 1378...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mesa vertical; Acurácia; Tecnologia de aplicação.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200015

Calibration of angles of nozzles and deposition of an axial-flow sprayer on dwarf cashew
Provedor de dados: 70
Autores: Mion,Renildo L.; Sousa,Beatriz M. de; Cordeiro,Igor M.; Sombra,Weberte A.; Duarte,José M. de L.; Lucas,Fidel C. B.
The study aimed to determine an optimum angle for the nozzles axial-flow sprayers a deposition for better vertical distribution focused on cashew. In laboratory tests were conducted adjusting the angle of the nozzle axial-flow sprayers. The experimental design was randomized blocks in a 2x3 factorial with four replications. The treatment for this test were two settings (with and without the adjustment of the angles of the nozzles ) and tree application volumes 273, 699 and 954 L ha-¹.The study was conducted in an orchard of dwarf cashew, with eight years of age. It was concluded that the volumetric distribution profile showed better vertical distribution uniformity when the angles of the nozzles were regulated for the canopy, the adjustment of the angles...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fruit; Deposition; Vertical patternator.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400020