Consulta: creatorFacets:"Matter,Juliana M."
Registros recuperados: 1
Data/hora: 09/06/2024 09:05:43

Anaerobic co-digestion of hatchery waste and wastewater to produce energy and biofertilizer - Batch phase
Provedor de dados: 91
Autores: Matter,Juliana M.; Costa,Mônica S. S. de M.; Costa,Luiz A. de M.; Pereira,Dercio C.; Varennes,Amarílis de; Tessaro,Dinéia.
ABSTRACT Aiming to evaluate different wastewaters in the anaerobic co-digestion (ACoD) of hatchery wastes, a batch test was conducted in bench horizontal digesters. At the end of the process, the potential production of biogas and methane was calculated as well as the chemical composition (macro- and micronutrients) of the effluent and the concentrations of methane and carbon dioxide gas at 60 days. The monitoring of the process included observations of the reduction of the organic carbon, chemical oxygen demand, and total (TS) and volatile solids (VS), as well as the variation of pH and electrical conductivity (EC). The results showed that the mixing between the hatchery fresh waste and swine wastewater (T4) and among fresh hatchery waste, water from the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogas; Methane; Swine wastewater; Slaughterhouse wastewater.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017000900651