Consulta: creatorFacets:"Radier, Severine"
Registros recuperados: 1
Data/hora: 17/06/2024 07:13:55

Recovery of valuable soluble compounds from washing waters generated during small fatty pelagic surimi processing by membrane processes
Provedor de dados: 5
Autores: Dumay, Justine; Radier, Severine; Barnathan, Gilles; Berge, Jean-pascal; Jaouen, Pascal.
This work focuses on the treatment of washing waters coming from surimi manufacturing using ultrafiltration technology at a laboratory scale. Four membrane materials (poly-ether sulfone, polyacrilonytrile, poly vinylidene fluoride and regenerated cellulose) and 5 Molecular Weight Cut-Off (from 3 to 100 kDa) have been studied at bench laboratory scale using the pilot Rayflow (R) 100, commercialised by Rhodia Orelis. The investigation deals with the ability for membranes to offer a high retention of biochemical compounds (proteins and lipids). Results obtained during adsorption tests showed that the regenerated cellulose material seems to be the most appropriate with regards to pore size reduction due to the protein-adsorption. During the ultrafiltration of...
Tipo: Text
Palavras-chave: Fish oil; Regenerated cellulose; Surimi wastewater; Enzymatic hydrolysis; Ultrafiltration.
Ano: 2008
URL: http://archimer.ifremer.fr/doc/2008/publication-4359.pdf