Consulta: creatorFacets:"Rosa,Luiz Mauro G."
Registros recuperados: 1
Data/hora: 13/06/2024 04:41:46

Calibrated heat-pulse method for the assessment of maize water uptake
Provedor de dados: Scientia Agricola
Autores: Santos,Antonio Odair; Bergamaschi,Homero; Rosa,Luiz Mauro G.; Bergonci,João Ito.
Plant water requirements are important aspects of crop production to be determined in the field, in order to judiciously manage crop water usage. Water uptake by field grown maize (Zea mays L.), under well-watered conditions was verified with the heat-pulse system. The temperature difference between two radially inserted thermocouples, one 9 mm above and the other 4 mm below a heater piercing the maize stem, was measured every 0.3 seconds following emission of a heat-pulse. Comparisons of the heat-pulse system outputs, lysimetric measurement and transpiration model estimates were monitored on an hourly and daily basis. At normal and low atmospheric demand daily and hourly values of heat-pulse outputs and lysimetric measurement showed good agreement. Hourly...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sap flow; Transpiration; Heat-pulse.
Ano: 2000
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162000000100006