Consulta: creatorFacets:"Togola, Anne"
Registros recuperados: 3
Data/hora: 12/06/2024 17:10:16

A Prospective Surveillance Network for improved identification of contaminants of emerging concern (CECs) and testing of innovative monitoring tools in France
Provedor de dados: 5
Autores: Staub, Pierre-françois; Dulio, Valeria; Gras, Olivier; Perceval, Olivier; Ait-aïssa, Selim; Aminot, Yann; Budzinski, Hélène; Lardy-fontan, Sophie; Lestremau, François; Miège, Cécile; Munschy, Catherine; Togola, Anne; Vulliet, Emmanuelle.
Tipo: Text
Ano: 2019
URL: https://archimer.ifremer.fr/doc/00623/73463/72746.pdf

Passive samplers for monitoring priority micropollutants in surface waters: a national scale study
Provedor de dados: 5
Autores: Mathon, Baptiste; Togola, Anne; Mazella, Nicolas; Lardy-fontan, Sophie; Dabrin, Aymeric; Ghestem, Jean-philippe; Tixier, Celine; Gonzalez, Jean-louis; Botta, Fabrizio; Miège, Cécile.
The implementation of the Water Framework Directive (WFD) requires the monitoring of micropollutants in the aquatic environments to prevent any damages to both human health and ecosystems. In this context, a number of organic and inorganic compounds have been selected as priority pollutants and their measurement is necessary to ensure that water-quality standards are maintained (EC, 2008; EC, 2013; EC, 2015). For two decades, passive sampling methods have been developed for the monitoring of organic and inorganic compounds. Passive samplers allow measuring these compounds at trace levels by accumulation and concentration over long-term exposure. Moreover, the use of integrative passive samplers (IPS) allows a better representativeness of measurements...
Tipo: Text
Ano: 2017
URL: https://archimer.ifremer.fr/doc/00618/73057/72185.pdf

Comparison of five integrative samplers in laboratory for the monitoring of indicator and dioxin-like polychlorinated biphenyls in water
Provedor de dados: 5
Autores: Jacquet, Romain; Miege, Cecile; Smedes, Foppe; Tixier, Celine; Tronczynski, Jacek; Togola, Anne; Berho, Catherine; Valor, Ignacio; Llorca, Julio; Barillon, Bruno; Marchand, Philippe; Coquery, Marina.
This study aimed at evaluating and comparing five integrative samplers for the monitoring of indicator and dioxin-like polychlorinated biphenyls (PCBs) in water: semi-permeable membrane device (SPMD), silicone rubber, low-density polyethylene (LDPE) strip, Chemcatcher and a continuous-flow integrative sampler (CFIS). These samplers were spiked with performance reference compounds (PRCs) and then simultaneously exposed under constant agitation and temperature in a 200 L stainless steel tank for periods ranging from one day to three months. A constant PCB concentration of about 1 ng·L−1 was achieved by immersing a large amount of silicone rubber sheets (“dosing sheets”) spiked with the target PCBs. The uptake of PCBs in the five samplers showed overall good...
Tipo: Text
Palavras-chave: Integrative samplers; Polychlorinated biphenyls; Water monitoring; Time weighted average concentration; Modeling.
Ano: 2014
URL: http://archimer.ifremer.fr/doc/00162/27317/25962.pdf