Consulta: subjectFacets:"Amande"
Registros recuperados: 1
Data/hora: 06/06/2024 01:28:16

Caractéristiques de dragues et pêcheries
Provedor de dados: 5
Autores: Pitel, Mathilde; Berthou, Patrick; Fifas, Spyros.
Basically, a dredge is a bottom-towed gear and consists of a metal frame with a blade or teeth, to dig into the sediment and extract the shelled molluscs, and a mesh bag to collect the catch. Whereas hand dredging is observed on some intertidal beds (Donax trunculus in France), the use of dredge generally needs a fishing boat. There is a great diversity of dredge types, with specific designs used to target different species in particular beds:   Manual dredges for Donax (Donax trunculus), Warty venus (Venus verrucosa) and clams (Venerupis pulastra, Ruditapes sp)   Dredges for King scallops (Pecten maximus)   Dredges for Warty venus (Venus verrucosa)   Dredge for Queen scallops (black and white, Chlamys varia and Chlamys opercularia)   Dredges for small...
Tipo: Text
Palavras-chave: Management; Environmental impact; Spisula; Bittersweet palourdi; Fishing boat; Clam; Dredge; Brittany; Gestion; Impact environnemental; Spisula; Amande; Navire de pêche; Drague; Bretagne.
Ano: 2001
URL: http://archimer.ifremer.fr/doc/2001/rapport-4608.pdf