Consulta: subjectFacets:"Enegy in agriculture Standalone"
Registros recuperados: 1
Data/hora: 11/06/2024 18:49:23

Performance study of a standalone direct pumping photovoltaic system used for drip irrigation
Provedor de dados: 111
Autores: HARKANI, ASSIA; El Aissaoui, Abdellah.
This paper aims to study performances of a standalone photovoltaic pumping system confronted to actual behaviour of incident irradiance. The system is based on a photovoltaic generator, a MPPT/ DC-DC converter, and a diaphragm DC motor pump connected to calibrated ( Flow versus Pressure) orifices, simulating small drip irrigation network, mounted in parallel scheme to vary the pump operating point according to timely varied irradiance. The result showed  that daily trend of solar irradiance influence considerably operating behaviour of the pump, consequently the performance of the standalone PV system is affected as there is inadequation between charges of the PV generator and the DC pump.  The hydraulic effeciency trends showed a dispersion and varying...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural engineering; Enegy in agriculture Standalone; Photovoltaic pumping system; Performances; Irradiance; Efficiency; MPPT; DC pump.
Ano: 2019
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/4822