Consulta: subjectFacets:"Gas flow"
Registros recuperados: 1
Data/hora: 03/06/2024 04:42:26

Portable flow board for storage of fruits and vegetables in mini-chambers with controlled atmosphere
Provedor de dados: Engenharia Agrícola
Autores: Carmelo,Luis G. P.; Becaro,Aline A.; Ferreira,Marcos D.; Calbo,Adonai G.
ABSTRACT A portable flow board system was developed in the present study with the aim to facilitate lab-scale experiments of controlled atmosphere (CA) with fruits and vegetables. This sturdy flow board combines ease fabrication, low cost and gas economy. Its functionality is provided by manifolds and gas mixers. Each gaseous component is supplied by a gas cylinder through a differential valve of adjusted pressure control, generally at 6 kPa, and forced through 13 standardized restrictors coupled to each manifold output. Controlled atmospheres are then formed with one, two or three gases in 13 gas mixers affixed to the flow board base, which are further conducted through flexible tubes to storage mini-chambers that can also be used to study metabolic...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Flow-board; Flux control; Gas flow; Method; Gas mixer; Restriction.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601105