Consulta: subjectFacets:"In situ chemical analyzer"
Registros recuperados: 1
Data/hora: 16/06/2024 20:07:43

Long-Term In Situ Survey of Reactive Iron Concentrations at the EMSO-Azores Observatory
Provedor de dados: 5
Autores: Laes-huon, Agathe; Cathalot, Cecile; Legrand, Julien; Tanguy, Virginie; Sarradin, Pierre-marie.
A study of the temporal dynamics of iron concentrations and temperature on a faunal assemblage at the Lucky Strike vent was performed using the Tempo ecological module at the EMSO-Azores deep-sea observatory. The CHEMINI in situ analyzer was implemented on this structure to determine reactive iron concentrations in unfiltered seawater samples along with a temperature probe. Stability tests were performed on the CHEMINI analyzer before deployment (optical module, hyperbaric tests, and deep-sea calibration) for long-term in situ analysis of reactive iron (six months, 2013–2014) at the Tour Eiffel active edifice. Recorded daily, the in situ standard (25 \mu mol.L {}^{-1} ) showed excellent reproducibility (1.07%, n=522 ), confirming satisfactory analytical...
Tipo: Text
Palavras-chave: Deep-sea observatory; Hydrothermal vent; In situ chemical analyzer; Iron; Monitoring the Mid-Atlantic Ridge (MoMAR).
Ano: 2016
URL: http://archimer.ifremer.fr/doc/00342/45275/46432.pdf