Consulta: subjectFacets:"Simplex optimization"
Registros recuperados: 1
Data/hora: 05/06/2024 01:31:10

Application of modified simplex on the development of a preconcentration system for cadmium determination in sediments, food and cigarettes
Provedor de dados: 42
Autores: SANTOS,QUEILA O.; MORENO,ISLANIA; SANTOS,LEANDRO DOS; SANTOS,ALDENOR G.; SOUZA,VALDINEI S.; BEZERRA,MARCOS A.
A modified simplex algorithm was used to optimize a system of preconcentration for cadmium determination in samples of sediments, cigarettes and food using flame atomic absorption spectrometry. The preconcentration system is based on the sorption of cadmium in a minicolumn packed with Amberlite XAD-2 resin functionalized with 3,4-dihydroxybenzoic acid (DHB). The optimized variables were pH and sampling flow rate and the optimum conditions found for these variables were, respectively 8.7 and 8.8 mL min-1. The developed system showed a preconcentration factor of 15.3, detection limit of 0.49 µg L-1, quantification limit of 1.65 µg L-1 and precision expressed as relative standard deviation (% RSD, n=10) of 5.9. The accuracy of the method was checked by...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Simplex optimization; Preconcentration; Cadmium; Sediments; Cigarettes; Food.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0001-37652016000300791