Consulta: subjectFacets:"Wave analysis"
Registros recuperados: 5
Data/hora: 03/06/2024 09:57:00

High Resolution Altimetry Reveals New Characteristics of the December 2004 Indian Ocean Tsunami
Provedor de dados: Institutional Archive of Ifreme (ArchiMer)
Autores: Ablain, Michaël; Dorandeu, Joël; Le Traon, Pierre-yves; Sladen, Anthony.
The Indian Ocean tsunami, which occurred on December 26, 2004, was the first to be clearly observed using satellite altimeters. The wave amplitude observed in deep-ocean by TOPEX and Jason-1 was close to 60 cm about 2 hours after the earthquake. Envisat crossed the tsunami wave 3h15 after the earthquake and measured a 35 cm wave. Even though it flew over the tsunami 7h20 after the earthquake, GFO still observed a wave close to 20 cm. To better extract the tsunami signal from altimeter measurements, a specific ocean variability mapping technique is used. This technique proves to be mandatory for discriminating tsunami waves from other ocean signals. Altimeter signals are then compared with those derived from the CEA (Commissariat à l'Energie Atomique) model...
Tipo: Text
Palavras-chave: Wave analysis; Tsunamis; Earthquakes; Sea level changes; Satellite altimetry.
Ano: 2006
URL: http://archimer.ifremer.fr/doc/2006/publication-1174.pdf

Análisis de las olas en la costa central del Ecuador
Provedor de dados: Ocean Docs: e-repository of  publications
Autores: Allauca, S.; Cardin, V.
El presente trabajo consiste en la recopilación de datos de olas existentes en las zonas ya mencionadas, con el propósito de analizar la climatología de olas en cada una de ellas, tratando de relacionarlas en forma conjunta, así como determinar la variabilidad de los parámetros de olas en los diferentes sitios. En este artículo se detalla la estadística básica de las alturas significativas y períodos medios, el análisis de la refracción de oleaje, las relaciones entre los parámetros medidos y las características de las olas extremas ó alturas significativas que pueden esperarse en un determinado período de tiempo.
Tipo: Journal Contribution
Palavras-chave: Wave analysis; Wave data; Climatology; Climatology; Http://aims.fao.org/aos/agrovoc/c_1671.
Ano: 1987
URL: http://hdl.handle.net/1834/2136

Características  del régimen de olas en San Cristóbal Islas Galápagos
Provedor de dados: Ocean Docs: e-repository of  publications
Autores: Espín, S.M.; Nath, J.
Un estudio de las características del régimen del oleaje en la isla San Cristóbal fue realizado durante el período comprendido entre diciembre de 1990 y diciembre de 1991. Los datos fueron obtenidos con un sensor de presion instalado en el veril de 9 m. en Bahía Naufragio, obteniéndose un registro de 2436 datos de alturas significativas y períodos medios. Del análisis de las series de alturas, períodos y los vientos de la región se determinó que las olas registradas corresponden a un régimen estacional ya que las de mayor altura y menores períodos se presentaron durante la época seca (de Mayo a Septiembre), con la intensificación de los vientos del sur y sureste, y las de menor amplitud y grandes períodos en la época húmeda. El arrecife de Schiavoni que se...
Tipo: Journal Contribution
Palavras-chave: Pressure sensors; Wave period; Wave height; Wave analysis; Oceanic islands.
Ano: 1992
URL: http://hdl.handle.net/1834/2184

A General formatting system for geo-referenced data. vol. 3: Standard subsets of GF3
Provedor de dados: Ocean Docs: e-repository of  publications
Tipo: Book
Palavras-chave: Oceanography; Geophysical data; Sea level; Sea level measurement; Wave analysis; Wave data; Wave height; Wave measurement; Sea surface; Drifting data buoys; Bathymetric data; Bathymetry; Mean sea level; Sea level; Http://aims.fao.org/aos/agrovoc/c_34115.
Ano: 1996
URL: http://hdl.handle.net/1834/2798

Analysis of wave observations and wave transformations in abu-qir, egypt
Provedor de dados: Ocean Docs: e-repository of  publications
Autores: Sharaf El-Din, S.H.; Abdallah, A.M.; Shereet, S.M.
Wave observations taken during 1986 in Abu-Qir Bay were statistically analyzed to calculate the wave parameters describing the sea state (significant wave height, wave period and predominant direction). On both sides of Rosetta promontory, the transformed wave parameters at break line (breaker height, breaker depth and crest angle) were calculated in terms of the predominant values of the significant wave height, period and direction using ACES software package. Breaker type and closure depth along Rosetta coast were also predicted. Generally, the wave effect in the bay was varying in intensity and direction in accordance with the prevailing wind. The average annual wave height and period are about 0.94 m and 6.5 s, respectively. Throughout the year, the...
Tipo: Journal Contribution
Palavras-chave: Physical Studies; Wave analysis.
Ano: 2006
URL: http://hdl.handle.net/1834/1449