Data/hora: 03/06/2024 15:11:50

Provedor de dados: 	Engenharia Agrícola	
País: 	Brazil	
Título: 	Portable flow board for storage of fruits and vegetables in mini-chambers with controlled atmosphere	
Autores: 	Carmelo,Luis G. P.; Becaro,Aline A.; Ferreira,Marcos D.; Calbo,Adonai G.	
Data: 	2015-12-01	
Ano: 	2015	
Palavras-chave: 	Flow-board; Flux control; Gas flow; Method; Gas mixer; Restriction.	
Resumo: 	ABSTRACT A portable flow board system was developed in the present study with the aim to facilitate lab-scale experiments of controlled atmosphere (CA) with fruits and vegetables. This sturdy flow board combines ease fabrication, low cost and gas economy. Its functionality is provided by manifolds and gas mixers. Each gaseous component is supplied by a gas cylinder through a differential valve of adjusted pressure control, generally at 6 kPa, and forced through 13 standardized restrictors coupled to each manifold output. Controlled atmospheres are then formed with one, two or three gases in 13 gas mixers affixed to the flow board base, which are further conducted through flexible tubes to storage mini-chambers that can also be used to study metabolic consumption and production of gaseous components. The restrictors used in the flow gaseous components were manufactured from microhematocrit test-type capillary glass tubes following the hot forming method under continuous air flow. The portable flow board showed to be low cost and simple post-harvest equipment that allows preparing controlled atmospheres in open systems with stable composition and flow, in a manner similar to traditional flow boards with control of gas escape by barostats.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601105	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/1809-4430-Eng.Agric.v35n6p1105-1116/2015	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.35 n.6 2015	
Fonte: 	info:eu-repo/semantics/openAccess