Data/hora: 27/07/2024 01:42:00

Provedor de dados: 	70	
País: 	Brazil	
Título: 	USE OF ACTIVE OPTICAL SENSOR IN THE CHARACTERISTICS ANALYSIS OF THE FERTIGATED BRACHIARIA WITH TREATED SEWAGE	
Autores: 	Santos,Gilmar O.; Rosalen,David L.; Faria,Rogério T. de.	
Data: 	2017-12-01	
Ano: 	2017	
Palavras-chave: 	Forage production estimation; GreenSeeker; Terrestrial remote sensing.	
Resumo: 	ABSTRACT Through the use of remote sensing, the productivity and the nutritional state of the plants can be estimated in relation to the nitrogen doses due to the modification of the canopy reflectance. In this study, values of the normalized difference vegetation index (NDVI) obtained by a terrestrial optical sensor were correlated with productivity and contents of nitrogen (N) and of foliar crude protein (CP) of Brachiaria brizantha cv. Marandu, fertigated with doses of sewage treatment effluent (STE) The NDVI average rates of the forage were obtained by the active terrestrial sensor (GreenSeeker) before the harvests that were realized every 28 days in 2014. Five fertigated treatments with the following fractions of STE in water were evaluated: E5 = 1.0; E4 = 0.87; E3 = 0.60; E2 = 0.31; and E1 = 0.11. During the 12 months of experiment, the treatment E5 received 1,132 kg ha-1 of N and the others received quantities proportional according to the application fractions defined in each treatment. The increasing application doses of STE resulted in higher yields of dry biomass and better leaf qualities in N and crude protein (CP). The productivity, the foliar N content and the NDVI index were increasing due to the gradual application of applied STE. There was a high linear correlation among the NDVI indexes and the productivity (r&gt;0.9256) and with the N content (r&gt;0.9570) and also for CP (r&gt;0.8421) and leaf N (r&gt;0.8339), demonstrating that the method can be used to estimate forage productivity and quality.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601213	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/1809-4430-eng.agric.v37n6p1213-1221/2017	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.37 n.6 2017	
Fonte: 	info:eu-repo/semantics/openAccess