Consulta: subjectFacets:"Directional spectra"
Registros recuperados: 2
Data/hora: 26/07/2024 22:43:40

A suitable metocean hindcast database for the design of Marine energy converters
Provedor de dados: Institutional Archive of Ifreme (ArchiMer)
Autores: Boudiere, Edwige; Maisondieu, Christophe; Ardhuin, Fabrice; Accensi, Mickael; Pineau-guillou, Lucia; Lepesqueur, Jeremy.
Resource assessment as well as characterisation of site climatologies for the design of Marine Energy Converters requires data bases allowing an accurate description of the environmental forcing, especially waves and sea-states, on a high resolution grid. As a support to its research activities related to the development of marine renewable energies, Ifremer is building a specific hindcast data set for the assessment of sea-states climatologies. The main features of this database, built running an up-to-date configuration of the WaveWatch III® wave model on an unstructured grid extending from the South of the North Sea to the Bay of Biscay are presented here. Attention is given to the parameterization and forcing as well as the specific output data sets...
Tipo: Text
Palavras-chave: Directional spectra; Hindcast; WAVEWATCH III®; Marine renewable energy.
Ano: 2013
URL: http://archimer.ifremer.fr/doc/00164/27524/25710.pdf

Génération de bases de données océano-météorologiques pour l'élaboration de climatologies adaptées au dimensionnement des structures en mer
Provedor de dados: Institutional Archive of Ifreme (ArchiMer)
Autores: Boudiere, Edwige; Maisondieu, Christophe; Ardhuin, Fabrice; Accensi, Mickael; Pineau-guillou, Lucia; Lepesqueur, Jeremy.
The number of Marine Renewable Energy projects has rapidly raised over the last decades. Those require a refined description of environmental conditions, such as sea states, for resource assessments as well as for the conception of the Marine Energy Converters. Engineering studies require long-term data sets so as to assess temporal variability and extreme events of sea states at the scale of the implantation sites.,As a support to its research studies on Marine Renewable Energy, Ifremer is building a specific hindcast database, running the wave model WAVEWATCH III® on an unstructured grid. The wave model extends over the area from the South of the North Sea to the Bay of Biscay with a high spatial resolution and covers a 16 years period from 1996 to 2012....
Tipo: Text
Palavras-chave: Spectre directionnel; Hindcast; WAVEWATCH III®; Énergie marine renouvelable; Directional spectra; Hindcast; WAVEWATCH III®; Marine renewable energy.
Ano: 2013
URL: http://archimer.ifremer.fr/doc/00203/31418/29813.pdf