Data/hora: 27/07/2024 02:55:56

Provedor de dados: 	Institutional Archive of Ifreme (ArchiMer)	
País: 	France	
Título: 	Prévention de la biocorrosion des aciers inoxydables par modification de la composition chimique	
Autores: 	Lemaitre, C.; Hernandez, G.; Béranger, G.; Guezennec, Jean.	
Data: 	1990	
Ano: 	1990	
Resumo: 	By using electrochemical measurements and bacteria counting, we have verified that the added elements in an AISI 316L stainless steel, as poison allowing elements for the bacteria, like copper or arsenic, change the electrochemical properties versus the time, and modifie the structure of the bacterial population on the surface. Comparisons of the obtained results in synthetic sea water, sterilized or inoculated, and in natural sea water have permitted to observe very great differences versus the added elements. The use of sterilized natural sea water and then inoculated, gives results which permit to show the specific role of the aerobic and the anaerobic bacteria.	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	https://archimer.ifremer.fr/doc/00479/59107/61744.pdf

DOI:10.1051/mattech/199078120025

https://archimer.ifremer.fr/doc/00479/59107/	
Editor: 	EDP Sciences	
Formato: 	application/pdf	
Fonte: 	Matériaux &amp; Techniques (0032-6895) (EDP Sciences), 1990 , Vol. 78 , N. 12 , P. 25-33	
Fonte: 	info:eu-repo/semantics/openAccess

restricted use