Data/hora: 02/06/2024 17:45:07

Provedor de dados: 	111	
País: 	China	
Título: 	Kinematics of the Tined Combine Harvester Reel	
Autores: 	Moses Frank Oduori; University of Nairobi; Thomas Ochuku Mbuya; University of Nairobi; Jun Sakai; Kyushu University; Eiji Inoue; Kyushu University.	
Data: 	2012-09-27	
Ano: 	2012	
Palavras-chave: 	Combine harvester reel; Reel kinematics; Tine trajectory.	
Resumo: 	Although derivation of the kinematic equations of the combine harvester reel is readily achieved, certain inferences thereof suggest possible improvements in its kinematical design.  A mathematically computed reference value of the reel index (ratio of the product of the reel radius and rotational velocity to the reel advance velocity) is found to be larger than commonly recommended values.  The point, either spatial or temporal, within the cycle of reel motion, at which the tinebar should preferably enter the crop is discussed.  The pick-up performance of the tines is qualitatively analyzed and its possible improvement through redesign of reel tine kinematics is suggested. Keywords: combine harvester reel, reel kinematics, tine trajectory 	
Idioma: 	Inglês	
Identificador: 	http://www.cigrjournal.org/index.php/Ejounral/article/view/1577	
Editor: 	International Commission of Agricultural and Biosystems Engineering	
Relação: 	http://www.cigrjournal.org/index.php/Ejounral/article/download/1577/3122	
Formato: 	application/pdf	
Fonte: 	Agricultural Engineering International: CIGR Journal; Vol 14, No 3 (2012): CIGR Journal; 53-60	
Fonte: 	&lt;html /&gt;