Data/hora: 12/06/2024 03:58:15

Provedor de dados: | 111
País: | China
Título: | Data Points and Duration for Estimating Fuel Consumption of a Diesel Engine
Autores: | Dennis G. Watson; Tony V. Harrison; Richard W. Steffen.
Data: | 1969-12-31
Ano: | 1969
Resumo: | Accurate measurement of fuel consumption is required to quantify the efficiency of an engine orpredict emissions. As part of a larger project, accurate instantaneous fuel consumption data was required for a John Deere 4045T diesel engine. While establishing test criteria, it became evident that literature did not provide clear recommendations on the number of data points or time duration for data collection, for a diesel engine. Fuel consumption tests were conducted using up to 15 data points of percent fuel rate and up to 15 min of data collection. ased on statistical analysis of test results, at least 2 data points (0% and 100% of fuel rate) and 2 min of data collection are recommended for similar fuel-injected, diesel engine fuel rate tests. When a nonfuel injected engine is used, the Hogan et al. (2007) recommendation of at least 3 data points and 3.5 min of data collection should be followed.
Idioma: | Inglês
Identificador: | http://www.cigrjournal.org/index.php/Ejounral/article/view/1238
Editor: | International Commission of Agricultural and Biosystems Engineering
Formato: | application/pdf
Fonte: | Agricultural Engineering International: CIGR Journal; Volume X (2008)
Fonte: | &lt;html /&gt;