Data/hora: 02/06/2024 19:02:37

Provedor de dados: | 111
País: | China
Título: | APPLICATION OF SENSITIVITY  MEASURED PARAMETERS FOR MODELS EVALUTION.
Autores: | Nkakini, Silas Ovua.
Data: | 2015-09-25
Ano: | 2015
Palavras-chave: | AgriculturalEngineering; Farm Power and Machinery KEYWORDS : Tractive force  disc ploughing  loamy  sand  soil  modelling      sensitivity measurement   soil   moisture.
Resumo: | ABSTRACTSensitivity measured parameters was used to evaluate a better tractive efficiency  and tillage speeds. Predictive models for tractive force were developed using dimensional analysis. A disc ploughing tillage operations in a loamy sand soil, at tillage speeds of 1.94m/s, 2.22m/s and 2.5m/s were conducted, using trace tractor techniques.  The independent and dependent variables involved in the models were measured.  Developed mathematical models describing the tractors tyre-soil  interactions parameters were evaluated using sensitivity of measured parameters. The wheel  tractors tractive force models have sensitivity coefficients ranging from -0.01307 to 0.6705, -0.0058 to 0.7483 and -0.0024 to 0.8939  for ploughing , with all the independent variables  at 1,94m/s,2.22m/s  and 2.50m/s tillage speeds respectively. The results  obtained showed that a 10% change of independent variable (U1) would cause dependent variable (N) a negligible change.  The same negligible changes occur at 50%  and 100% , even at the maximum  change of  8.939  in ploughing  operations. These indicate that the sensitivity of developed predicted models to changes in the constituent independent variables are negligible and insignificant. Thus, sensitivity coefficients of  the tractive force models developed fit experimental data.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.cigrjournal.org/index.php/Ejounral/article/view/2849
Editor: | International Commission of Agricultural and Biosystems Engineering
Relação: | http://www.cigrjournal.org/index.php/Ejounral/article/view/2849/2148
Formato: | application/pdf

Fonte:

Agricultural Engineering International: CIGR Journal; Vol 17, No 3 (2015): CIGR Journal

1682-1130