Data/hora: 11/06/2024 01:00:40

Provedor de dados: 	111	
País: 	China	
Título: 	Experimental evaluation of substrate’s particle size of wheat and rice straw biomass on methane production yield	
Autores: 	Chandra, Ram; Takeuchi, H.; Hasegawa, T.; Vijay, V. K.	
Data: 	2015-06-23	
Ano: 	2015	
Palavras-chave: 	Bioenergy; Biogas production from lignocellulosic biomass wheat and rice straw; Biomass particle size; Anaerobic digestion; Methane yield.	
Resumo: 	This paper examines the effect of particle sizes in substrates on methane production yields of wheat and rice straw biomass without any other applied pretreatment. Anaerobic digestion of three different mean particle size (MPS) substrate of 1.5 mm, 0.75 mm, and 0.30 mm of wheat and rice straw biomass was carried out at 37 oC mesophilic temperature. The observed result revealed that mean particle size of 0.30 mm, and 0.75 mm had increased methane production yield by 4.7%, and 38.7%, respectively, compared to 1.50 mm particle size of wheat straw. However, in case of rice straw substrates the methane production yield was found 7.9%, and 13.0% higher, respectively, for mean particle size of 0.30 mm, and 0.75 mm, compared to 1.50 mm particle size. Mean particle size of 0.75 mm had yielded highest biogas as well as methane yields in both cases of biomass, however, wheat straw resulted into considerably higher methane yield than rice straw.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.cigrjournal.org/index.php/Ejounral/article/view/2844	
Editor: 	International Commission of Agricultural and Biosystems Engineering	
Relação: 	http://www.cigrjournal.org/index.php/Ejounral/article/view/2844/2103

http://www.cigrjournal.org/index.php/Ejounral/article/downloadSuppFile/2844/934	
Formato: 	application/pdf	
Fonte: 	Agricultural Engineering International: CIGR Journal; Vol 17, No 2 (2015): CIGR Journal

1682-1130