Data/hora: 08/06/2024 09:56:18

Provedor de dados: | 14
País: | Brazil
Título: | Comparação entre diferentes interpoladores na delimitação de bacias hidrográficas.
Autores: | REDIVO, A. L.; GUIMARÃES, R. F.; RAMOS, V. M.; CARVALHO JÚNIOR, O. A. de; MARTINS, E. de S.
Data: | 2008-03-05
Ano: | 2002
Palavras-chave: | Modelo digital; Hidrogeology; Digital model.; Bacia Hidrográfica; Hidrogeologia.; Geomorfologia; Geomorphology; Watersheds.
Resumo: | ABSTRACT: The morphometric parameters are of fundamental importance for the good operation of models, among them, the area of the basin to amount determined for each pixel stands out for releases use in hydrologic models used for the definition of saturation areas in the landscape and predictive models of mass movements. In this work three different ways are compared of obtaining the delimitation of hydrologic basins starting from a digital elevation model: a) Directly of DEM without any treatment type, being used of different interpolators types; b) Starting from the elimination of the depressions inherent of the interpolator that doesn't correspond to the nature and; c) Making DEM being used of the corresponding vectors the drainage net and water bodies, being eliminated, also, the depressions. The results show that the values obtained by the different processes possess significant discrepancy amongst themselves.
Tipo: | Documentos (INFOTECA-E)
Idioma: | Português

Identificador:

28473

http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/563076

Editor: | Planaltina, DF: Embrapa Cerrados, 2002.

Relação:

Embrapa Cerrados - Documentos (INFOTECA-E)

(Embrapa Cerrados. Documentos, 71).

Formato: | 20 p.