Data/hora: 03/06/2024 10:04:42

Provedor de dados: 	14	
País: 	Brazil	
Título: 	Considerações teóricas sobre o cálculo da resistência mecânica do solo à penetração determinada com penetrômetros dinâmicos.	
Autores: 	SÁ, M. A. C. de; SANTOS JÚNIOR, J. de D. G. dos.	
Data: 	2008-03-20	
Ano: 	2007	
Palavras-chave: 	Penetrômetro; Soil compactation.; Compactação do Solo; Manejo do Solo.; Penetrometers; Soil management.	
Resumo: 	ABSTRACT: The aim of this work was to describe an equations to calculate the soil mechanical impedance by dynamic penetrometers. The calculations regard two different equipments, including theoretical correction for the gravity aceleration. To obtain precision values of soil mechanics impedance, in research experiments, gauging all mass and weigths of the equipament was necessary. However, the gravity aceleration correction as a function of latitude and altitude was not important.	
Tipo: 	Documentos (INFOTECA-E)	
Idioma: 	Português	
Identificador: 	28617

http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/571933	
Editor: 	Planaltina, DF: Embrapa Cerrados, 2007.	
Relação: 	Embrapa Cerrados - Documentos (INFOTECA-E)

(Embrapa Cerrados. Documentos, 200).	
Formato: 	27 p.