Data/hora: 05/06/2024 06:32:21

Provedor de dados: 	19	
País: 	Japan	
Título: 	2輪駆動トラクタのけん引効率予測

Tractive Efficiency Prediction for a Two Wheel Drive Tractor	
Autores: 	大友, 功一; 岸本, 正; OHTOMO, Koichi; KISHIMOTO, Tadashi.	
Data: 	2000-03	
Ano: 	2000	
Palavras-chave: 	トラクタ; けん引力; けん引効率; 円すい指数; 予測モデル; Tractor; Drawbar pull; Tractive effciency; Cone index; Prediction model.	
Resumo: 	トラクタのけん引性能を評価するための一つの方法として, 2輪駆動トラクタのけん引効率の予測を行なった。予測精度を検討するために, トラクタの機体条件ならびに平均円すい指数からけん引効率等を予測すると共に, 土壌密度を変えた圃場でけん引性能試験を行ない実測データを収集した。けん引力およびけん引効率の実測値の予測値に対する偏差と予測最大値との比を偏差率として定義し求め, 予測精度を検討した。その結果, 全データの偏差率の平均値は, けん引力で0.07%, けん引効率で-0.29%となり, 提案モデルは高い精度で予測できることを示した。 A prediction of the tractive efficiency of a two-wheel drive tractor was conducted with tractor dimensions and average cone indexes. Experimental data in a field for the discussion of the prediction accuracy were obtained through tractor drawbar pull tests. The deviations of the measured data to the predicted one of drawbar pull and tractive efficiency were calculated，and the deviation rates which were defined as the ratio of the deviation to the predicted maximums of the drawbar pull and the tractive efficiency were obtained. The mean deviation rate of the drawbar pull and the tractive efficiency were 0.07% and -0.29% respectively. This reveals that reliable predictions for the tractive performance become possible.	
Idioma: 	Japonês	
Identificador: 	http://ir.obihiro.ac.jp/dspace/handle/10322/2955	
Editor: 	農業機械学会	
Formato: 	application/pdf	
Fonte: 	農業機械学会