Data/hora: 17/06/2024 09:57:09

Provedor de dados: | 27
País: | Belgium
Título: | Improvement of grain-size analyses using the automated SEDIGRAPH 5100
Autores: | Wartel, S.; Barusseau, J.-P.; Cornand, L.
Data: | 1995
Ano: | 1995
Resumo: | The method of analysing fine grained sediments is discussed and an improved technique using a water-glycerol solution of known density instead of water is proposed. Inaccuracies resulting from wet sieving may contribute to explain the observed difference between the pipette method and the Sedigraph 5100 analyses.
Tipo: | Info:eu-repo/semantics/book
Idioma: | Inglês
Identificador: | http://www.vliz.be/imisdocs/publications/136053.pdf
Formato: | application/pdf
Fonte: | %3Ci%3EStudiedocumenten+van+het+K.B.I.N.+%3D+Documents+de+Travail+de+l%27I.R.Sc.N.B.%3C%2Fi%3E%2C+80.+Koninklijk+Belgisch+Instituut+voor+Natuurwetenschappen%3A+Brussel.++28+pp.
Fonte: | info:eu-repo/semantics/openAccess