Data/hora: 06/06/2024 00:25:40

Provedor de dados: 	31	
País: 	United States	
Título: 	Subsurface Drip Irrigation Versus Center-Pivot Sprinkler for Applying Swine Effluent to Corn	
Autores: 	Carreira,   Rita I.; Stoecker,   Arthur L.; Epplin,   Francis M.; Hattey,   Jeffory A.; Kizer,   Michael A.	
Data: 	2008-10-01	
Ano: 	2006	
Palavras-chave: 	Aquifer depletion; Center-pivot sprinkler irrigation; Certainty equivalent; Corn irrigation; Mathematical programming; Risk; Stochastic optimization; Subsurface drip irrigation; Crop Production/Industries; C61; C65; Q12; Q30; Q53.	
Resumo: 	A risk-averse irrigated corn producer would be better off choosing the more expensive subsurface drip irrigation (SDI) over center-pivot sprinkler (CPS), given limited aquifer life and swine effluent and urea fertilization. A stochastic optimization using EPIC data maximized expected utility of 100 years' worth of net revenues for a quarter section. Phosphorus accumulation was more likely with the CPS than with the SDI but soil nitrogen was constant under both systems. SDI conserves more water than CPS per acre but depletes the aquifer faster because a greater area is irrigated. These results were invariant in the sensitivity analysis.	
Tipo: 	Journal Article	
Idioma: 	Inglês	
Identificador: 	http://purl.umn.edu/43783	
Relação: 	Journal of Agricultural and Applied Economics&gt;Volume 38, Number 03, December 2006	
Formato: 	14