Data/hora: 02/06/2024 16:54:23

Provedor de dados: | 32
País: | Mexico
Título: | Calidad de las aguas residuales urbano-industriales que riegan el Valle del Mezquital, Hidalgo, México
Autores: | Mendoza Saldivar, Isabel.
Data: | 2012-09-09
Ano: | 2009
Palavras-chave: | Salinidad; Sodicidad; RAS; PSI; CSR; Doctorado; Hidrociencias; Salinity; Sodicity; SAR; ESP; RSC.
Resumo: | En la actualidad se ha usado prácticamente toda agua disponible para satisfacer los requerimientos de humedad de los diferentes cultivos que activamente se explotan en la agricultura bajo riego. Cada vez más se utilizan hasta el límite las aguas superficiales y subterráneas de la más variada composición química y concentración de sales. En México, se riegan aproximadamente 180 000 ha en diferentes valles intermontanos del Valle del Mezquital con aguas residuales urbano-industriales que derivan de la zona metropolitana del Valle de México, prácticamente sin ningún tratamiento. En este trabajo de investigación se analizan y discuten los efectos de los elementos inorgánicos que afectan la calidad del agua de riego residual urbano-industrial de la red hidrográfica de Zumpango-Ixmiquilpan-Zimapán, que riegan el Valle del Mezquital, Hidalgo. Se analizan los problemas de salinidad y sodicidad de estas aguas, así como los contenidos de boro y ortofosfatos. Se encontró que los valores de la presión osmótica de las aguas residuales variaron como sigue: 16-24 kPa para fuentes de agua de manantiales y 55-186 kPa para las aguas residuales urbano-industriales de la red hidrográfica de Zumpango-Ixmiquilpan-Zimapán. La concentración total electrolítica de estas aguas varió de la siguiente manera: 135-4612 µ S cm-1. Altos niveles de sodio intercambiable propician la dispersión de las arcillas y afectan la infiltración del agua en los suelos. Los efectos de la sodicidad se evalúan con la relación de adsorción de sodio (RAS). Para ello se evaluaron las siguientes formulaciones RASor, RASaj y RASº. Se calcularon las sales hipotéticas en estas aguas y la composición salina resultó ser la siguiente: NaCl&gt;NaHCO3&gt;Mg(HCO3)2&gt;Ca(HCO3)2&gt;MgSO4. Estas aguas son: sódico-clorhídrico-bicarbonatadas. Los contenidos de boro fueron: 0.03-8.77 mg L-1. Los contenidos de ortofosfatos (PO43-) fueron: 0.05-34.61 mg L-1._________Nowadays, practically any available water is being used to satisfy the moisture requirements of the different crops that are actively being grown under irrigation conditions. Surface and underground waters are ever more being used to exhaustion, regardless of their varied chemical composition or concentration of salts. In Mexico, approximately 180 000 ha in different mountain valleys in the Valle del Mezquital are being irrigated with urban-industrial residual waters from the metropolitan zone of the Valle de Mexico, with practically no treatment. In the present research work are analyzed and discussed the effects of the inorganic elements that affect the quality of the urban-industrial residual waters used for irrigation in the Valle del Mezquital, Hidalgo, coming from the Zumpango-Ixmiquilpan-Zimapán water basin. Problems of salinity and sodicity in these waters are analyzed, as well as the contents of boron and orthophosphates. The values of osmotic pressure of the residual waters were found to vary as follows: 16-24 kPa for spring waters and 55-186 kPa for urban-industrial residual waters from the Zumpango-Ixmiquilpan-Zimapán water basin. The total electrolytic concentration of these waters varied as follows: 135-4612 µ S cm-1. High levels of exchangeable sodium favor the dispersion of clays and affect water infiltration into the soil. The effects of sodicity are evaluated with the sodium adsorption ratio (SAR). To do this, the following formulas were evaluated: SARor, SARaj, and SARº. Hypothetical salts were evaluated for these waters, and the saline composition turned out to be: NaCl&gt;NaHCO3&gt;Mg(HCO3)2&gt;Ca(HCO3)2&gt;MgSO4. The waters are: sodic-chlorhydric-bicarbonated. Boron contents were: 0.03-8.77 mg L-1. Orthophosphate (PO43-) contents were: 0.05-34.61mg L-1.
Tipo: | Tesis
Idioma: | Espanhol
Identificador: | http://hdl.handle.net/10521/1552