Data/hora: 10/06/2024 18:05:17

Provedor de dados: | 42
País: | Brazil
Título: | Dynamic Analysis of the Temperature and the Concentration Profiles of an Industrial Rotary Kiln Used in Clinker Production
Autores: | RODRIGUES,DIULIA C.Q.; SOARES JUNIOR,ATÍLIO P.; COSTA JUNIOR,ESLY F.; COSTA,ANDRÉA O.S.
Data: | 2017-12-01
Ano: | 2017
Palavras-chave: | Clinker; Dynamic analysis; Mathematical modelling; Rotary kiln.
Resumo: | ABSTRACT Cement is one of the most used building materials in the world. The process of cement production involves numerous and complex reactions that occur under different temperatures. Thus, there is great interest in the optimization of cement manufacturing. Clinker production is one of the main steps of cement production and it occurs inside the kiln. In this paper, the dry process of clinker production is analysed in a rotary kiln that operates in counter flow. The main phenomena involved in clinker production is as follows: free residual water evaporation of raw material, decomposition of magnesium carbonate, decarbonation, formation of C3A and C4AF, formation of dicalcium silicate, and formation of tricalcium silicate. The main objective of this study was to propose a mathematical model that realistically describes the temperature profile and the concentration of clinker components in a real rotary kiln. In addition, the influence of different speeds of inlet gas and solids in the system was analysed. The mathematical model is composed of partial differential equations. The model was implemented in Mathcad (available at CCA/UFES) and solved using industrial input data. The proposal model is satisfactory to describe the temperature and concentration profiles of a real rotary kiln.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0001-37652017000603123
Editor: | Academia Brasileira de Ciências
Relação: | 10.1590/0001-3765201720160661
Formato: | text/html
Fonte: | Anais da Academia Brasileira de Ciências  v.89 n.4 2017
Fonte: | info:eu-repo/semantics/openAccess