Data/hora: 01/06/2024 09:08:57

Provedor de dados: 	5	
País: 	France	
Título: 	Biofouling protection for marine environmental sensors	
Autores: 	Delauney, Laurent; Compere, Chantal; Lehaitre, Michel.	
Data: 	2010	
Ano: 	2010	
Resumo: 	These days, many marine autonomous environment monitoring networks are set up in the world. These systems take advantage of existing superstructures such as offshore platforms, lightships, piers, breakwaters or are placed on specially designed buoys or underwater oceanographic structures. These systems commonly use various sensors to measure parameters such as dissolved oxygen, turbidity, conductivity, pH or fluorescence. Emphasis has to be put on the long term quality of measurements, yet sensors may face very short-term biofouling effects. Biofouling can disrupt the quality of the measurements, sometimes in less than a week. Many techniques to prevent biofouling on instrumentation are listed and studied by researchers and manufacturers. Very few of them are implemented on instruments and of those very few have been tested in situ on oceanographic sensors for deployment of at least one or two months. This paper presents a review of techniques used to protect against biofouling of in situ sensors and gives a short list and description of promising techniques.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00008/11920/8626.pdf

DOI:10.5194/os-6-503-2010	
Editor: 	Copernicus Gesellschaft Mbh	
Relação: 	http://archimer.ifremer.fr/doc/00008/11920/	
Formato: 	application/pdf	
Fonte: 	Ocean Science (1812-0784) (Copernicus Gesellschaft Mbh), 2010 , Vol. 6 , N. 2 , P. 503-511	
Fonte: 	Author(s) 2010. European Geosciences Union