Data/hora: 06/06/2024 14:07:01

Provedor de dados: | 5
País: | France
Título: | Modelisation numerique du flambage de panneaux sandwich raidis
Autores: | Batoz, J; Quesnel, T.
Data: | 1992-12
Ano: | 1992
Palavras-chave: | Ship technology; Composite materials; Modelling; Mathematical models; Numerical analysis; Eléments finis; Plaque coque; Flambage; Structure sandwich; Matériau composite.
Resumo: | This paper presents a numerical method for the buckling analysis of stiffened sandwich panels for ship building with composite materials. The formulation of a multi-layered quadrilateral finite element of a plane shell including transverse shear effects is presented. Some classical tests allow the performance of this element to be evaluated for composite plates. Then an explanation is given for a method used for analyzing the buckling of panels.
Tipo: | Text
Idioma: | Francês
Identificador: | http://archimer.ifremer.fr/doc/1992/acte-1074.pdf
Editor: | Actes de colloques. Ifremer. Brest [ACTES COLLOQ. IFREMER.]. 1992
Relação: | http://archimer.ifremer.fr/doc/00000/1074/
Formato: | application/pdf