Data/hora: 17/06/2024 03:18:07

Provedor de dados: 	5	
País: 	France	
Título: 	DORIS Software. New Tool to Process Sound Velocity Profiles	
Autores: 	Sinquin, Jean-marc; Lurton, Xavier; Vignaud, Christophe; Mathieu, Gregory; Bisquay, Herve.	
Data: 	2016-05-25	
Ano: 	2016	
Resumo: 	Hydrographic and geosciences surveys, using acoustic devices, need to use accurate water sound velocity profiles. Because the acoustic path depends on the sound velocity profile (SVP), the use of the most accurate SVP is one of the keys to conducting effective surveys (with multibeams, for instance). To date, the existing software available does not answer to both the needs of efficiency and simplicity (sometimes not so easy to operate, sometimes not so accurate). DORIS provides a handy freeware to post-process SVP for the hydrographic communities.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00339/45065/44473.pdf

http://archimer.ifremer.fr/doc/00339/45065/	
Editor: 	Geomares Publishing	
Formato: 	application/pdf	
Fonte: 	Hydro International (1385-4569) (Geomares Publishing), 2016-05-25 , Vol. 20 , N. 4 , P. 22-25	
Fonte: 	2016, Geomares Publishing, The Netherlands All rights reserved

info:eu-repo/semantics/openAccess

restricted use