Data/hora: 07/06/2024 01:04:57

Provedor de dados: | 5
País: | France
Título: | New modelling of submarine gravity flows: application to the Nice collapse in 1979.
Autores: | Hugot, Alexandre; Joseph, Philippe; Savoye, Bruno; Zaleski, Stéphane.
Data: | 2001-07
Ano: | 2001
Palavras-chave: | France; 1979 Nice airport collapse; Inverse problem; Flow object; Turbidity current; Gravity flow.
Resumo: | We propose to apply in this note a simple mathematical model for the sedimentation of gravity deposits in deep water. An inverse method has been developed in order to characterize the parameters associated with the submarine flow. This method also provides the initial conditions, which constitute a major uncertainty in geoscience modelling. Application of the inverse method to the 1979 Nice air-port collapse (southern France), constrained by cable breaks and/or deposit thicknesses, leads, for example, to the estimation of the initial volume and/or the physical parameters of the flow (friction coefficient, modified turbulent Schmidt number, etc.). The application of the model to this real case shows that only the simultaneous inversion of dynamic (cable break times) and sedimentological (deposit) data allows a satisfactory reconstruction of the flow.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/2001/publication-787.pdf

DOI:10.1016/S1251-8050(01)01606-8

Editor: | Elsevier
Relação: | http://archimer.ifremer.fr/doc/00000/787/
Formato: | application/pdf
Fonte: | Comptes Rendus de l'Academie des Sciences - Series IIA - Earth and Planetary Science (1251-8050) (Elsevier), 2001-07 , Vol. 333 , N. 2 , P. 133-139
Fonte: | 2001 Académie des sciences/Éditions scientifiques et médicales Elsevier SAS. All rights reserved