Data/hora: 14/06/2024 00:06:27

Provedor de dados: | 5
País: | France
Título: | Development of a Mass Sensitive Quartz Crystal Microbalance (QCM)-Based DNA Biosensor Using a 50 MHz Electronic Oscillator Circuit
Autores: | Garcia-martinez, Gonzalo; Alonso Bustabad, Enrique; Perrot, Hubert; Gabrielli, Claude; Bucur, Bogdan; Lazerges, Mathieu; Rose, Daniel; Rodriguez-pardo, Loreto; Farina, Jose; Compere, Chantal; Arnau Vives, Antonio.
Data: | 2011-08
Ano: | 2011
Palavras-chave: | DNA sequence detection; Quartz crystal microbalance; Electronic oscillator; Sensitivity; Frequency noise; Resolution.
Resumo: | This work deals with the design of a high sensitivity DNA sequence detector using a 50 MHz quartz crystal microbalance (QCM) electronic oscillator circuit. The oscillator circuitry is based on Miller topology, which is able to work in damping media. Calibration and experimental study of frequency noise are carried out, finding that the designed sensor has a resolution of 7.1 ng/cm(2) in dynamic conditions (with circulation of liquid). Then the oscillator is proved as DNA biosensor. Results show that the system is able to detect the presence of complementary target DNAs in a solution with high selectivity and sensitivity. DNA target concentrations higher of 50 ng/mL can be detected.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/00044/15487/12886.pdf

DOI:10.3390/s110807656

Editor: | Mdpi Ag
Relação: | http://archimer.ifremer.fr/doc/00044/15487/
Formato: | application/pdf
Fonte: | Sensors (1424-8220) (Mdpi Ag), 2011-08 , Vol. 11 , N. 8 , P. 7656-7664
Fonte: | 2011 by the authors; licensee MDPI, Basel, Switzerland.